Engineering - Landscape Architecture - Surveying
7 Waldo Street, St. Augustine, FL 32084 | 904.826.1334 | www.matthews.dccm.com
mdg.cei@dccm.com
LICENSE #26535, LB8590, LA6666877
M

Site Notes

N/A

Corrected since last report

N/A

Observations

•·161@Mi
l	l	Structure functioning as designed.

fif®M±l1i
15	25	Paver settling.Correct or monitor for worsening condition.Repair if progresses to trip hazard.

16	26	Minimal separation between concrete flags in sidewalk. Suggest shaving down to reduce change in elevations for trip hazard.Monitor in future inspections.

23	34	Bench support is loose.Monitor under future inspections.

24	35	Bench support is loose.Monitor in future inspections.
Matthews	
24015 Double Branch CDD Field Report#12025-06-23

Observations

25	36	Depression and cracking in tennis court surface.Monitor in future inspections.

26	37	Cracking in basketball court surface. Observe in future inspections.

20	30	Degraded pavement/depression near inlet in parking lot.Observe under future reviews.

fiMii:t
11	21	Photo taken of pond for record purposes, only in comparison for future visits.

12	22	Photo taken of pond for record purposes, only in comparison for future visits.

13	23	Photo taken of pond for record purposes, only in comparison for future visits.

Needs Action

•·160i6Mi
	2.	4	Weir block by debris.Removed debris and vegetation to allow weir to operate as designed.

	2.	5	Weir blocked by debris.Removed debris, clean out structure to allow weir to operate as designed.

	2.	6	Control structure weir is blocked by debris.Remove debris to allow weir to function as designed.

	6.	8	Control structure weir blocked by vegetation. Remove vegetation to allow control structure to function as designed.

	6.	11	Confirmed clog at both inlets and discharging MES. CDD to facilitate vac truck to clear the pipe lines.This should be addressed immediately.
Matthews	
24015 Double Branch CDD
Field Report#12025-06-23

Needs Action

	6.	20

•aNiM:t

	6.	16

fiflVM½Mi
Outflow appears to be bypassing aluminum weir plate underneath through original concrete weir.Tightening the aluminum plate against the concrete weir for a watertight seal will be required for proper control structure, design function.

Pond bank washout possibly related to homeowner irrigation. CDD to reach out to homeowner and run corner sprinkler to see if that is causing the washout from overspray of the area or a leak in the irrigation system. This pin location was formerly classified as a possible animal burrow has been cleared now that the issue is confirmed to not be a burrow.

14	24	Stairs appear to be settling and separating from pavers. Suggest inspection for stability.

21	32	Bench support is loose.Re-stabilize/ secure for support.

ffiihifi1i

	2.	7

Misc

5	7

l1ffl9
	6.	19
Erosion in pond bank.Re-stabilize to protect against erosion.

Erosion in pond bank.Re-stabilize to protect against erosion.

Exposed rust with sharp edges.Rusted support corner for walkway landing.Repair to protect from sharp edges and monitor for structural support in future inspections.

17	27	Railing support is loose needs to be re-secured.

18	28	Missing blue reflector in roadway to identify hydrant location. Add blue reflector to roadway.

22	33	Exposed metal rust with sharp edges.Remove and re-secure trashcan.

f§Mii:t
7	11	Confirmed clog at both inlets and discharging MES.CDD to facilitate vac truck to clear the pipe lines.This should be addressed immediately.

Matthews	
24015 Double Branch CDD Field Report#12025-06-23

Map Overview

Matthews	
24015 Double Branch CDD Field Report#12025-06-23

	2.	Needs Action

Pin Type: General

Categories:
f•lfiiiM·•
Location:

Notes:

Branden J Marcinell June 10, 2025 3:06 PM EDT
Control structure weir is blocked by debris. Remove debris to allow weir to function as designed.

Photos:
Created by:

Branden J Marcinell

Jun 10, 2025 at 3:06 pm EDT

Matthews	
24015 Double Branch CDD
Field Report #12025-06-23

	2.	Needs Action

Pin Type: General

Categories:
f§jij•@§j@	Misc
Location:
Created by:

Branden J Marcinell

Jun 10, 2025 at 2:29 pm EDT

Notes:

Branden J Marcinell June 10, 2025 2:29 PM EDT
Erosion in pond bank. Re-stabilize to protect against erosion.

Photos:

Matthews	
24015 Double Branch CDD Field Report#12025-06-23

19	Needs Action

Pin Type: General

Categories:

Location:
Created by:

Branden J Marcinell

Jun 10, 2025 at 2:41 pm EDT

Notes:

Branden J Marcinell June 10, 2025 2:41PM EDT
Exposed rust with sharp edges. Rusted support corner for walkway landing.Repair to protect from sharp edges and monitor for structural support in future inspections.

Photos: